**Executed only once**

0 – use internal delay configure via code

a – Toggle LED on and off.

1,2,3,4 – Toggle sensor heater 1, 2, 3 or 4 on and off.

r – cycle temperature and pressure resolution (256 > 512 > 1024 > 2048 > 4096 > 8192 > 256 > …). It doesn’t change humidity resolution.

T – temperature on demand

P – pressure on demand

H – humidity on demand

**Kept in memory**

t – broadcast temperature

p – broadcast pressure

h – broadcast humidity

u – broadcast temperature (fast mode)

q – broadcast pressure (fast mode)

s - stop